<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.54" y2="0" width="0" layer="20"/>
<wire x1="35.54" y1="0" x2="35.54" y2="9.83" width="0" layer="20"/>
<wire x1="35.54" y1="9.83" x2="0" y2="9.83" width="0" layer="20"/>
<wire x1="0" y1="9.83" x2="0" y2="0" width="0" layer="20"/>
<text>oontz.org</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SIMHOLDER3">
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOT95P270X145-5N">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP12SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Connectors" package="SIMHOLDER3" value="SIMHOLDER3"/>
<element name="." library="Microchip_By_element14_Batch_1" package="SOT95P270X145-5N" value="24LC08BT-I/OT">
<attribute name="PACKAGE" value="SOT23-5"/>
<attribute name="OC_NEWARK" value="62K0577"/>
<attribute name="MPN" value="24LC08BT-I/OT"/>
<attribute name="SUPPLIER" value="MICROCHIP"/>
<attribute name="OC_FARNELL" value="1556163"/>
</element>
<element name="VCC" library="testpad" package="TP12SQ" value="TPSQTP12SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCL" library="testpad" package="TP12SQ" value="TPSQTP12SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VSS" library="testpad" package="TP12SQ" value="TPSQTP12SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDA" library="testpad" package="TP12SQ" value="TPSQTP12SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="5"/>
<contactref element="." pad="2"/>
<contactref element="." pad="5"/>
<contactref element="VSS" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="." pad="1"/>
<contactref element="SCL" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="." pad="3"/>
<contactref element="SDA" pad="TP"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="2"/>
<contactref element="." pad="4"/>
<contactref element="VCC" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
